1. By adding the RID’s into the wrangler child\_create event call
2. By adding a rule that listened for the wrangler child\_initialized event. Which meant that the child was created and ready to receive the profile\_updated event
3. I made a python script calling either the sky/event for making event calls and the sky/cloud for function calls on the ruleset
4. I would store all the children sensor ECI in the management ruleset and in the rule listening for wrangler child\_initialized I would pass them the ECI of their brethren and save them on the children picos. (After having had added a rule to listen for brethren ECI update or something along those lines) then they can iterate through the ecis and talk to their brothers as the project required. 